board <- 1;
derivative <- 1;
outputvariant <- 1;
function BeginWizard()
{
	// this is the text that will appear in the start (intro) page
	local intro_msg = _T(	"Welcome to the new ARM application wizard!\n" +
				"This wizard will guide you to create a new ARM application.\n\n" +
				"Please click \"Next\" to proceed.");

	local ARM_boards = _T(	"ARM-eval7t;" +
					"ek-at91sam7a3;" +
					"lpd-lh7a404;" +
					"olimex-at91sam7sx;" +
					"olimex-lpc213x;" +
					"phyCORE-AT91M55800;" +
					"phyCORE-LPC2294;" +
					"phyCORE-PXA255;"
					);
	// intro
	Wizard.AddInfoPage(_T("ConsoleIntro"), intro_msg);
	// select project name and path
	Wizard.AddProjectPathPage();
	// select compiler and configurations
	Wizard.AddCompilerPage(_T(""), _T("armelf*"), false, false);
	// select language
	Wizard.AddGenericSingleChoiceListPage(_T("ARMBoards"), _T("Please select your ARM evaluation board."), ARM_boards , board);

	// Targetconfiguration for ARM
	Wizard.AddGenericSingleChoiceListPage(_T("ARM_eval7t_Config"), _T("Please select the configuration you want to use."), _T("default"), derivative);
	Wizard.AddGenericSingleChoiceListPage(_T("ek_at91sam7a3_Config"), _T("Please select the configuration you want to use."), _T("Code in ROM;Code in RAM"), derivative);
	Wizard.AddGenericSingleChoiceListPage(_T("lpd_lh7a404_Config"), _T("Please select the configuration you want to use."), _T("default"), derivative);
	Wizard.AddGenericSingleChoiceListPage(_T("olimex_at91sam7sx_Config"), _T("Please select the configuration you want to use."), _T("at91sam7s32;at91sam7s64;at91sam7s128;at91sam7s256"), derivative);
	Wizard.AddGenericSingleChoiceListPage(_T("olimex_lpc213x_Config"), _T("Please select the configuration you want to use."), _T("lpc2132;lpc2134;lpc2136;lpc2138"), derivative);
	Wizard.AddGenericSingleChoiceListPage(_T("phyCORE_AT91M55800_Config"), _T("Please select the configuration you want to use."), _T("default;ROM;RAM 512kB;RAM 1MB"), derivative);
	Wizard.AddGenericSingleChoiceListPage(_T("phyCORE_LPC2294_Config"), _T("Please select the configuration you want to use."), _T("default;ROM;RAM 1MB"), derivative);
	Wizard.AddGenericSingleChoiceListPage(_T("phyCORE_PXA255_Config"), _T("Please select the configuration you want to use."), _T("default"), derivative);

//	Wizard.AddGenericSingleChoiceListPage(_T("OutputVariant"), _T("Please select the content of your project.\nPlease note: Empty projects are only compilable\nafter adding files!"), _T("Empty project;Compilable project with dummyfiles"), outputvariant);
}
//
//------------------------------------------------------------------------------
//
function OnLeave_ARMBoards(fwd)
{
	if (fwd)
	{
		board = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	}
	return true;
}

function OnGetNextPage_ARMBoards()
{
	switch (Wizard.GetListboxSelection(_T("GenericChoiceList")))
	{
		case 0:
			return _T("ARM_eval7t_Config");
			break;
		case 1:
			return _T("ek_at91sam7a3_Config");
			break;
		case 2:
			return _T("lpd_lh7a404_Config");
			break;
		case 3:
			return _T("olimex_at91sam7sx_Config");
			break;
		case 4:
			return _T("olimex_lpc213x_Config");
			break;
		case 5:
			return _T("phyCORE_AT91M55800_Config");
			break;
		case 6:
			return _T("phyCORE_LPC2294_Config");
			break;
		case 7:
			return _T("phyCORE_PXA255_Config");
			break;
	}
	return _T("")
}

function OnLeave_ARM_eval7t_Config(fwd)
{
	if (fwd)
	{
		derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	}
	return true;
}

function OnGetPrevPage_ARM_eval7t_Config()
{
	return _T("ARMBoards");
}

function OnGetNextPage_ARM_eval7t_Config()
{
	derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	return _T("OutputVariant")
}

function OnLeave_ek_at91sam7a3_Config(fwd)
{
	if (fwd)
	{
		derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	}
	return true;
}

function OnGetPrevPage_ek_at91sam7a3_Config()
{
	return _T("ARMBoards");
}

function OnGetNextPage_ek_at91sam7a3_Config()
{
	derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	return _T("OutputVariant")
}

function OnLeave_lpd_h7a404_Config(fwd)
{
	if (fwd)
	{
		derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	}
	return true;
}

function OnGetPrevPage_lpd_lh7a404_Config()
{
	return _T("ARMBoards");
}

function OnGetNextPage_lpd_lh7a404_Config()
{
	derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	return _T("OutputVariant")
}

function OnLeave_olimex_at91sam7sx_Config(fwd)
{
	if (fwd)
	{
		derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	}
	return true;
}
function OnGetPrevPage_olimex_at91sam7sx_Config()
{
	return _T("ARMBoards");
}
function OnGetNextPage_olimex_at91sam7sx_Config()
{
	derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	return _T("OutputVariant")
}

function OnLeave_olimex_olimex_lpc213x_Config(fwd)
{
	if (fwd)
	{
		derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	}
	return true;
}
function OnGetPrevPage_olimex_lpc213x_Config()
{
	return _T("ARMBoards");
}
function OnGetNextPage_olimex_lpc213x_Config()
{
	derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	return _T("OutputVariant")
}

function OnLeave_phyCORE_AT91M55800_Config(fwd)
{
	if (fwd)
	{
		derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	}
	return true;
}
function OnGetPrevPage_phyCORE_AT91M55800_Config()
{
	return _T("ARMBoards");
}
function OnGetNextPage_phyCORE_AT91M55800_Config()
{
	derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	return _T("OutputVariant")
}

function OnLeave_phyCORE_LPC2294_Config(fwd)
{
	if (fwd)
	{
		derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	}
	return true;
}
function OnGetPrevPage_phyCORE_LPC2294_Config()
{
	return _T("ARMBoards");
}
function OnGetNextPage_phyCORE_LPC2294_Config()
{
	derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	return _T("OutputVariant")
}

function OnLeave_phyCORE_PXA255_Config(fwd)
{
	if (fwd)
	{
		derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	}
	return true;
}
function OnGetPrevPage_phyCORE_PXA255_Config()
{
	return _T("ARMBoards");
}
function OnGetNextPage_phyCORE_PXA255_Config()
{
	derivative = Wizard.GetListboxSelection(_T("GenericChoiceList"));
	return _T("OutputVariant")
}


//
//------------------------------------------------------------------------------
//
function GetFilesDir()
{
//	if (outputvariant == 0)
//	{
//		return _T("");
//	}

	switch (board)
	{
		case 0:
			return _T("arm") + wxFILE_SEP_PATH + _T("files") + wxFILE_SEP_PATH + _T("ARM-eval7t");
			break;

		case 1:
			return _T("arm") + wxFILE_SEP_PATH + _T("files") + wxFILE_SEP_PATH + _T("ek-at91sam7a3");
			break;

		case 2:
			return _T("arm") + wxFILE_SEP_PATH + _T("files") + wxFILE_SEP_PATH + _T("lpd-lh7a404");
			break;

		case 3:
			return _T("arm") + wxFILE_SEP_PATH + _T("files") + wxFILE_SEP_PATH + _T("olimex-at91sam7sx");
			break;

		case 4:
			return _T("arm") + wxFILE_SEP_PATH + _T("files") + wxFILE_SEP_PATH + _T("olimex-lpc213x");
			break;

		case 5:
			return _T("arm") + wxFILE_SEP_PATH + _T("files") + wxFILE_SEP_PATH + _T("phyCORE-AT91M55800");
			break;

		case 6:
			return _T("arm") + wxFILE_SEP_PATH + _T("files") + wxFILE_SEP_PATH + _T("phyCORE-LPC2294");
			break;

		case 7:
			return _T("arm") + wxFILE_SEP_PATH + _T("files") + wxFILE_SEP_PATH + _T("phyCORE-PXA255");
			break;
	}

}
//
//------------------------------------------------------------------------------
//
function SetupProject(project)
{
	local target;
	local i;

	// NOTE: Major compiler system drawback here.
	// Until it is redesigned to allow easier compiler settings,
	// we have to check the compiler's ID and set options for different compilers...
	// We make things easier for scripts, by providing a few predefined functions
	// to setup common settings like "debug", "warnings", etc.
	// These functions are located in <templates_path>/common_functions.script.
	// If you add other commonly used functions or bug-fix anything in that file,
	// please share it with us :)

	// enable compiler warnings (project-wide)
	WarningsOn(project, Wizard.GetCompilerID());
	DebugSymbolsOn(project, Wizard.GetCompilerID());
	OptimizationsOn(project, Wizard.GetCompilerID());

	// Add subdirectories for includes
	project.AddIncludeDir(_T("src"));
	project.AddIncludeDir(_T("h"));

	project.AddCompilerOption(_T("-fno-common"));
	project.AddLinkerOption(_T("-Wl,-Map,map.txt"));

	SetupDerivative(derivative,project);

	// We setup the targets using SetupTarget() which is conveniently called by Code::Blocks
	// if we register this wizard as wizTarget type :)
	// This means that this very wizard can be used both as wizProject *and* as wizTarget ;)

	//configure default target
	target = project.GetBuildTarget(_T("default"));

	if (IsNull(target))
		target = project.AddBuildTarget(_T("default"));

	SetupTarget(target, true);

	for (i = 0; i < project.GetFilesCount(); i++)
	{
		if ((project.GetFile(i).relativeFilename.Matches(_T("*S"))) || (project.GetFile(i).relativeFilename.Matches(_T("*s"))))
		{
			project.GetFile(i).compile = true;
			project.GetFile(i).link = true;
		}
	}
	// all done!
	return true;
}
//
//------------------------------------------------------------------------------
//
function SetupTarget(target,is_debug)
{
	if (IsNull(target))
		return false;

	local projectname = GetProjectManager().GetActiveProject().GetTitle();
	target.SetTargetType(ttConsoleOnly);

	target.SetTargetFilenameGenerationPolicy(1, 1);
	target.SetOutputFilename(target.GetTitle() + wxFILE_SEP_PATH + projectname + _T(".elf"));

	target.SetObjectOutput(target.GetTitle());

	switch (board)
	{
		case 2:
			target.AddCommandsAfterBuild(_T("arm-elf-objcopy --change-section-lma .text+0xC0000000 --change-section-lma .rom_vectors+0xC0000000 --change-section-lma .rodata+0xC0000000 --change-section-lma .jcr+0xC0000000 --change-section-lma .data+0xC0000000 --change-start 0xC0000000 ") + target.GetTitle() + wxFILE_SEP_PATH + projectname + _T(".elf"));
			break;
		case 7:
			target.AddCommandsAfterBuild(_T("arm-elf-objcopy --change-section-lma .text+0xA0000000 --change-section-lma .rom_vectors+0xA0000000 --change-section-lma .rodata+0xA0000000 --change-section-lma .jcr+0xA0000000 --change-section-lma .data+0xA0000000 --change-start 0xA0000000 ") + target.GetTitle() + wxFILE_SEP_PATH + projectname + _T(".elf"));
			break;
	}

	if (is_debug)
	{
		// enable debugging symbols for this target
		DebugSymbolsOn(target, Wizard.GetCompilerID());
	}

	return true;
}


function SetupDerivative(derivative,project)
{
	switch (board)
	{
		case 0:// ARM-eval7t
			project.AddCompilerOption(_T("-mcpu=arm7tdmi"));
			project.AddCompilerOption(_T("-DARM_EVAL7T"));
			project.AddCompilerOption(_T("-D__NO_CTOR_DTOR_SUPPORT__"));
			project.AddCompilerOption(_T("-DUSE_IRQ"));
			project.AddLinkerOption(_T("-mcpu=arm7tdmi"));

			switch (derivative)
			{
				case 0:
					project.AddLinkerOption(_T("-T ld/target.ld"));
				break;
			}
			break;

		case 1:// ek-at91sam7a3
			project.AddCompilerOption(_T("-mcpu=arm7tdmi"));
			project.AddCompilerOption(_T("-DEK_AT91SAM7A3"));
			project.AddCompilerOption(_T("-D__NO_CTOR_DTOR_SUPPORT__"));
			project.AddCompilerOption(_T("-DUSE_IRQ"));
			project.AddLinkerOption(_T("-mcpu=arm7tdmi"));

			switch (derivative)
			{
				case 0:
					project.AddLinkerOption(_T("-T ld/target.ld"));
				break;
				case 1:
					project.AddLinkerOption(_T("-T ld/targetRAM.ld"));
				break;
			}
			break;

		case 2:// lpd-lh7a404
			project.AddCompilerOption(_T("-mcpu=arm9tdmi"));
			project.AddCompilerOption(_T("-DLPD_LH7A404"));
			project.AddCompilerOption(_T("-DENABLE_ICACHE"));
			project.AddCompilerOption(_T("-DENABLE_DCACHE"));
			project.AddCompilerOption(_T("-DUSE_IRQ"));
			project.AddLinkerOption(_T("-mcpu=arm9tdmi"));

			switch (derivative)
			{
				case 0:
					project.AddLinkerOption(_T("-T ld/target.ld"));
				break;
			}
			break;

		case 3:// olimex-at91sam7sx
			project.AddCompilerOption(_T("-mcpu=arm7tdmi"));
			project.AddCompilerOption(_T("-DOLIMEX_AT91SAM7SX"));
			project.AddCompilerOption(_T("-D__NO_CTOR_DTOR_SUPPORT__"));
			project.AddCompilerOption(_T("-DUSE_IRQ"));
			project.AddLinkerOption(_T("-mcpu=arm7tdmi"));

			switch (derivative)
			{
				case 0:
					project.AddLinkerOption(_T("-T ld/target_s32.ld"));
				break;
				case 1:
					project.AddLinkerOption(_T("-T ld/target_s64.ld"));
				break;
				case 2:
					project.AddLinkerOption(_T("-T ld/target_s128.ld"));
				break;
				case 3:
					project.AddLinkerOption(_T("-T ld/target_s256.ld"));
				break;
			}
			break;

		case 4:// olimex-lpc213x
			project.AddCompilerOption(_T("-mcpu=arm7tdmi"));
			project.AddCompilerOption(_T("-DOLIMEX_LPC213X"));
			project.AddCompilerOption(_T("-D__NO_CTOR_DTOR_SUPPORT__"));
			project.AddCompilerOption(_T("-DUSE_IRQ"));
			project.AddLinkerOption(_T("-mcpu=arm7tdmi"));

			switch (derivative)
			{
				case 0:
					project.AddLinkerOption(_T("-T ld/target_2132.ld"));
				break;
				case 1:
					project.AddLinkerOption(_T("-T ld/target_2134.ld"));
				break;
				case 2:
					project.AddLinkerOption(_T("-T ld/target_2136.ld"));
				break;
				case 3:
					project.AddLinkerOption(_T("-T ld/target_2138.ld"));
				break;
			}
			break;

		case 5:// phyCORE-AT91M55800
			project.AddCompilerOption(_T("-mcpu=arm7tdmi"));
			project.AddCompilerOption(_T("-DPHYCORE_AT91M55800"));
			project.AddCompilerOption(_T("-DUSE_IRQ"));
			project.AddLinkerOption(_T("-mcpu=arm7tdmi"));

			switch (derivative)
			{
				case 0:
					project.AddLinkerOption(_T("-T ld/target.ld"));
				break;
				case 1:
					project.AddLinkerOption(_T("-T ld/targetROM.ld"));
				break;
				case 2:
					project.AddLinkerOption(_T("-T ld/targetRAM_512kB.ld"));
				break;
				case 3:
					project.AddLinkerOption(_T("-T ld/targetRAM_1MB.ld"));
				break;
			}
			break;

		case 6:// phyCORE-LPC2294
			project.AddCompilerOption(_T("-mcpu=arm7tdmi"));
			project.AddCompilerOption(_T("-DPHYCORE_LPC2294"));
			project.AddCompilerOption(_T("-DUSE_IRQ"));
			project.AddLinkerOption(_T("-mcpu=arm7tdmi"));

			switch (derivative)
			{
				case 0:
					project.AddLinkerOption(_T("-T ld/target.ld"));
				break;
				case 1:
					project.AddLinkerOption(_T("-T ld/targetROM.ld"));
				break;
				case 2:
					project.AddLinkerOption(_T("-T ld/targetRAM_1MB.ld"));
				break;
			}
			break;

		case 7:// phyCORE-PXA255
			project.AddCompilerOption(_T("-mcpu=xscale"));
			project.AddCompilerOption(_T("-DPHYCORE_PXA255"));
			project.AddCompilerOption(_T("-DFAST_CLOCK"));
			project.AddCompilerOption(_T("-DENABLE_ICACHE"));
			project.AddCompilerOption(_T("-DUSE_IRQ"));
			project.AddLinkerOption(_T("-mcpu=xscale"));

			switch (derivative)
			{
				case 0:
					project.AddLinkerOption(_T("-T ld/target.ld"));
				break;
			}
			break;
	}
}
